{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":20,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":157,"n_cols":5,"rows_kept":157,"merged":[[1,0,1,4]],"flags":["formulas_cached_only"]}
[]
["CHECKS"]
[1,null,"Enough Fuel on Fuel Tank"]
[]
[2,null,"Check Fluid Level for Front & Rear Brakes AND Functioning"]
[{"$nulls":3},"Check","Top-Up"]
{"$rows_empty":23}
[3,null,"Tires Pressure & Wear"]
[{"$nulls":3},"Single - Front 26.1 psi  -- Rear 33.4 psi"]
[{"$nulls":3},"Double - Front 29.0 psi -- Rear 40.6 psi"]
{"$rows_empty":8}
[4,null,"Functioning Parking Light, Headlamp, Turn Indicators, Stop Light & License Plate Light"]
[]
[5,null,"Engine Oil Level"]
[{"$nulls":3},"Check","Replace"]
{"$rows_empty":24}
[6,null,"Coolant Level"]
{"$rows_empty":21}
[7,null,"Schock Absorber"]
[{"$nulls":3},"1--Min Driver"]
[{"$nulls":3},"2--Max Driver"]
[{"$nulls":3},"3--Min Driver Plus Passanger"]
[{"$nulls":3},"4--Max Driver Plus Passanger"]
[]
[]
[]
[]
[]
[8,null,"Hub Oil"]
[{"$nulls":3},"Check","Replace"]
{"$rows_empty":22}
[9,null,"Air Filter"]
{"$rows_empty":9}
[10,null,"Fuses"]
{"$rows_empty":21}
[11,null,"Battery"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}